BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x73
Card Placement Error

Default definition: |  | ALARM + NOPROG + EXTERN + ACTIVE |
Used by block: |  | SU |
Category: |  | MAINTENANCE |

Some card position in the system has E2-data stored, that does not match the actual card type.

- D1:
- D2: Lowest card position, that did not match
- D3: Undefined
- D4: Undefined

#### Recommended action

Use BMS to check, which board positions cause the problem and evaluate the type of fault for the respective board position. If the relevant board position (placing) is intentional, use the ‘update board position’ function, otherwise the relevant boards are to be placed in their correct positions.

Revision: F © Ericsson Enterprise 2003