BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1016
Reroute on no answer ?

The command is used for direct in-dialing and private trunks for rerouting of incoming calls to the rerouting position if the destination required does not answer.

If “No” is programmed ringing will continue at the selected extension.

For rerouting to take place it is necessary the rerouting position has been programmed, see commands 1103 Reroute position at day and 1104 Reroute position at night.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003