BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0107
Break-in allowed ?

On a call to a busy extension it may be possible (permitted) to intrude (break in) on the ongoing call, i.e. effect intrusion.

This command states whether others may intrude on a call in which the extension is a participant.

Only those extensions (PABX-operators) whose facility category permits intrusion are allowed to initiate this facility. See command 3004 Intrusion.

Note

When this command, for an analogue extension, is set to NO, outgoing ISDN calls will have bearer capabilities changed to 3.1 kHz audio. This may be used if a fax or modem is connected.

In some ISDN networks this may not be allowed.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003