BusinessPhone Communication Platform 4.0
Dialogs

## Transmission – Group 1-7

This dialog shows the parameters for transmission group 1 to 7.

To access the dialog, open the “System” menu in the Configuration directory tree. Next open the “System parameters” submenu and click on “Transmission”. Select “Group 1-7” in the context menu.

The following commands are available:

2710 |  | Transmission Group 0

Note

The dialog depends on the system configuration.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |

See Facility Descriptions:

- Analogue Telephone (111/15534-ASB 150 02 Uen).
- Trunk (486/15534-ASB 150 02 Uen).

Revision: A © Ericsson Enterprise 2003