BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0xAE
Free CIL Buffer Check Failed

Default definition: |  | ERROR |
Used by block: |  | OS |
Category: |  | MAINTENANCE |

This code is only used, when the periodic resource check, initiated by the supervision programs, failed. The warning indicates that the maximum number of free buffers, located in the data map of the CIL application, that has been available since the last check, is smaller than the anticipated number. The cause can be, that the external CIL hardware is turned off or unable to receive the CIL information because of any other reason.

- D1:
- D2: CIL data map number
- D3: Undefined
- D4: Undefined

#### Recommended action

Verify the connection of the external (peripheral) equipment and the programming of the relevant IO-channel.

Revision: F © Ericsson Enterprise 2003