BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8512
Exit position

An external caller who is diverted to the individual mailbox system may be connected to another extension instead of leaving a message, i. e. is the directory number the external caller will be rerouted to. For each tenant group an exit position is specified.

Furthermore, an internal or external caller who is connected to the message system to retrieve messages from an extension may be connected to another extension.

In the following traffic cases the call is rerouted as well:

- Timeout when waiting for response from an external caller (by pressing a key).
- If the external caller cannot be connected to the message system, e.g. no VMU-HD installed.

If no directory number is specified and the caller is external, the rewriting position of the relevant trunk is used (see commands 1103 Reroute position at day, 1104 Reroute position at night). In case of an internal caller, the call is disconnected.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003