BusinessPhone Communication Platform 4.0
Commands > Commands 7000...7999

## 7801
RSU-group reservation

With this command it is possible to reserve each RSU-group (Register Signalling Unit) for one register signalling application. The 2 different applications are traffic register signalling and voice services. If none of these is specified, both will be handled.

Values:

0 = |  | No RSU-groups reserved (default)

1 = |  | Reserved for traffic register signalling

2 = |  | Reserved for voice services

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003