BusinessPhone Communication Platform 4.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 97 ELCTRL

00h ELCCWTONE |  | Order call-waiting tone to instrument |
01h ELCKEYREL |  | Control of INSTRTYPE messages |
02h ELCLINEBR |  | Order line break |
03h ELCINDMODEC |  | Instrument mode for ELUC |
04h ELCINDMODED |  | Instrument mode for ELUD |
05h ELCFUNC |  | Function control |
06h ELCTONE |  | Start/stop tone sending |
07h ELCANAMODE |  | Mode control (ELUA) |
08h ELCLEVELD |  | Loudspeaker and ear piece level (ELUD) |
09h ELCDIR |  | Associated directory number |
0Ah ELCLCDPAR |  | Special cordless display characters |

Revision: PD2 © Ericsson Enterprise 2003