BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0177
Initiate callback corporate network ?

The command defines if an extension is allowed to request a call back from an extension within the corporate network.

Default data: NO = CN Call Back not allowed

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003