BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x91
Extended Tracelog Warning

Default definition: |  | ALARM |
Used by block: |  | OM |
Category: |  | DESIGNER |

This warning is not caused by a specific error, but is used as an optional signal in the EXTENDED TRACE mechanism to show that the selected event has occurred. The warning data differs for the warning trace and the state trace.

Warning trace

- D1: Data from the original warning
- D2: Data from the original warning
- D3: Data from the original warning
- D4: Data from the original warning

State trace

- D1: 0
- D2: 0
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003