BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x9D
Active Alarm Failed

Default definition: |  | ALARM |
Used by block: |  | OM |
Category: |  | MAINTENANCE |

The code is used by the active alarm function.

- D1: Type of error

- 00h: Used by the ‘test call’ function.
- 01h: Sendlimit reached. Nothing more will be sent this day.
- 10h: No timer received. The ‘active’ function will be disabled. No attempt to send this alarm has been made.
- 11h: Unable to seize port, SEIZNAK received, nothing sent.
- 12h: No connection, CONEND received, nothing sent.
- 13h: No answer to alarm call, no CONRDY received.

- D2: Number of alarms in EEPROM buffer (D1 = 01H)
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003