BusinessPhone Communication Platform 4.0
Facilities

## Text Mode

## Definition

Text can in certain modes be entered from the EXECUTIVE Telephone and the OPERATOR’s Console.

Text is entered via the key pad.

## Use

Text can be entered in the following cases:

- TEXT INFORMATION
- TEXT MESSAGE
- TELEPHONE DIRECTORY
- HOTEL RECEPTION, see Hotel (241/155 34-ASB 150 02 Uen).
- SYSTEM PROGRAMMING, see Facility Description (155 34-ASB 150 02 Uen)

## Operation

In those modes in which writing is permitted this is indicated by a cursor on the display.

In the text mode the keys on the EXECUTIVE Telephone possess the key functions shown below:

Key 2-9 can be used for the letter A-Z.

Each key has three or more letters allocated to the key.

National characters can be found behind the 1-key.

Special characters . , ! ? are found behind the *-key.

+-key is used to step to next position or for space.

--key is used to erase the digit under the cursor.

When a key is pressed in the text mode, the leftmost letter will be shown on the display.

If the key is pressed a second time, the next letter will appear. When the key is pressed after the rightmost letter the digit for the key is shown.

If a new key is pressed the cursor will automatically move to the next position.

If one wants to write two letters subsequently on the same key the +-key must be pressed between the two letters.

Some examples (“-” indicates consecutive depressions of the same key, “,” indicates that a new key is pressed):

To write “JOHN” the following keys have to be pressed: 5,6-6-6,4-4,6-6

To write “ROSS”: 7-7-7,6-6-6,7-7-7-7,+,7-7-7-7

## Capacity/Limitations

None

## Programming

None

## Equipment

EXECUTIVE Telephone or OPERATOR’s Console.

Revision: C © Ericsson Enterprise 2003