BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2035
Predicted call duration

This command defines the duration in seconds for which the predicted call cost will be calculated. The calculation is done for each carrier who offers the desired destination.

Range for call duration: 10 digits incl. decimal point

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003