BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1008
Camp-on to answering position ?

The command states whether it is permitted to camp on the trunk to a specified answering position, if this position is busy.

For the incoming call to be allowed to camp on, the answering position must also allow camp-on.

For direct in-dialing (DID) calls that are diverted to an alternative answering position, camp-on will take place even if the command is set to “No”.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003