BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1014
Result tones to parent exchange ?

The command is used to determine whether a result tone shall be sent to the parent exchange. This applies both to incoming and outgoing calls.

Valid data: Yes / No

Default data: Yes

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003