BusinessPhone Communication Platform 4.0
Start Of Operation ASB 150 02

## General description

These instructions are intended for setting up the ASB 150 02 system where the included units or the entire system have/has been subjected to factory end testing before delivery to the installation site.

This document covers tests for the following:

- extension lines
- trunk lines
- MDF for extension and trunk lines
- programmed functions
- information to the customer

The instructions describe the test procedures that are to be used.

The ASB 150 02 introduces with the release 9 the functionality of exchanging boards of similar type and exact configuration without the need of turning off the mains power to restart the system. This functionality is known under the term "hot swapping".

### Supplementary documents

- Installation Instruction (1531‑BDV 113 08 Uen)
- Installation Instruction (1531‑BDV BS 101 01 Uen)
- Fault Tracing Information (1545‑ASB 150 02 Uen)
- RASC User Guide EN/LZT BS 102 023

### Fault locating

If a fault is discovered, the directions given in “Fault Tracing Information” are to be followed.

Revision: G © Ericsson Enterprise 2003