BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6014
Dialled number

The command determines the digits constituting the dialled number.

The following characters may be used:

0-9 |  | Digit to be sent

*,# |  | Character to be sent

- |  | Wait for second dial tone

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003