BusinessPhone Communication Platform 4.0
Installation Instruction ASB 150 02 > Boards For ASB 150 02

## BTU-B (ROF 157 5121/_)

#### Applies for indices 1 and 3

The BTU-B provides connection for up to 8 physical links and every physical link can be configured as a S- or T-interface in point-to-point or multi-point mode. On the S-interface every link provides remote power feeding with 40V/50 mA = 2W and connection for up to 8 terminals.

Revision: A © Ericsson Enterprise 2003