BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2343
Traffic check at break-in

This command states how the traffic group check should be executed at intrusion.

Alternatives:

0 = |  | It is only necessary that the intruding party is open to call the busy extension.

1 = |  | The intruding party is open to call the busy extension and must also be open to call or receive call from the third party.

2 = |  | The traffic group has to be open in both directions between all parties before the intrusion is allowed.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003