BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2028
Ringtime for internal calls

This command defines the time needed for sending a Ringing Signal to an extension in case of an internal call.

Valid values for this command are 0-255.

With 0, no supervision is active.

All other values state the ringing time in seconds.

If a call is diverted because of an unanswered call the stipulated time is reseted and the supervision restarted.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003