BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0165
Diversion on no reply to slave ?

The command defines whether or not a diversion on no reply to an associated slave extension should be done. If the extension is a master and a member of a tandem configuration the command data shall be copied to the slave and blocked for the slave’s further use.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003