BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1308
PTS-signal from parent exchange = dial tone ?

The command states whether the proceed-to-send signal from the parent exchange is the dial tone.

(Command 1007 Break-in allowed ? states whether a proceed-to-send signal is sent by the parent exchange. See also command 1013 Dial tone to extension ?, which states whether a dial tone shall be sent to the extension.)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003