BusinessPhone Communication Platform 4.0
Dialogs

## Restart History

This dialog shows the date and time of the latest restarts and the information saved when the system was restarted.

After a power up all RAM data areas are checked and cleared. This includes also the restart history area.

After a restart caused by the watchdog, a lot of important values and memory areas are copied to the restart history area: in this situation, these will not be cleared.

The first table displays date and type for up to six of the latest restarts, and information saved when the system was last restarted using the SUPERVISION function.

The SUPERVISION function restarts the system (i.e. it generates warning code 097, which is normally classed as STOP) when there is no response to the periodic supervision message that is sent to all cards, one by one. The data saved is for the current card. This is probably, but not necessarily, the faulty card. If there is a general communication failure on the system bus, or if a card has a fault that disturbs communication for other cards, this menu might point out the wrong card.

The next table displays the CPU restart history with the restart time and a list of active data, program and E1 maps.

The last received message is also shown.

The last table shows the data from the software interrupt interface parameter stack.

#### Dump to file

File name | Shows the file name to dump the log into
Append this dump to the existing file | If checked the log dump is added to the file with the given filename. If the check box is unchecked, a new file is created.

#### Actions

Dump |  | To dump all warning log entries to a file. |

See System Description (1551-ASB 150 02 Uen).

Revision: A © Ericsson Enterprise 2003