BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1036
Type of IBERCOM network connection

This command is used to define the type of ‘call class’ for some market specific traffic cases.

In case of Spanish market the external call setup for this call destination can be defined as an IBERCOM call with related parameters. The used network protocol on the actual (T-) link must be set to ‘network acc. to Spain’.

Value = |  | 0 |  | not specified (no IBERCOM network connection) |
|  | 1 |  | interuser IBERCOM network connection |
|  | 3 |  | intrauser IBERCOM network connection |

Initial value = 0

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003