BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x71
Individual Memory Not Sufficient

Default definition: |  | ALARM + NOPROG + EXTERN + ACTIVE |
Used by block: |  | SU |
Category: |  | MAINTENANCE |

SU could not allocate enough individual data memory. At start-up, SU tries to allocate data memory for all cards in the system, starting at card position 0. This warning is used, if not enough memory remains to satisfy the request of memory for the card.

- D1:
- D2: Card position, where the request failed
- D3: Undefined
- D4: Undefined

#### Recommended action

The only cure is to remove some card from the system.

Revision: F © Ericsson Enterprise 2003