BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0157
Diversion on no reply external
calls ?

The command defines whether or not a diversion on no reply on an external incoming call should be done.

If the extension is a master and a member of a tandem configuration the command data shall be copied to the slave and blocked for the slave's further use.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003