BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0xE2
Alarm Capacity Error

Default definition: |  | INFO |
Used by block: |  | AL |
Category: |  | MAINTENANCE |

This code is used, when a generated alarm was lost because the maximum storage capacity for alarms has been exceeded.

- D1: Directory number of the extension, where the alarm failed, high byte
- D2: Directory number of the extension, where the alarm failed, low byte
- D3: Alarm time, high byte
- D4: Alarm time, low byte

Revision: F © Ericsson Enterprise 2003