BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4701
Reference number for voice answer

With this command the reference number for voice answer is given. A total of three references per voice answer can be given.

Before a voice answer is programmed, the directory number must be created with the command 5408 Create voice answer. A total of 16 directory numbers can be created for voice answers.

The references are played in the order given in this command.

The directory number can be used as called to within the system.

The reference number are entered as: uuvvv

where

uu = |  | 01-28 |  | (01 = Voice announcement) |
|  |  |  | (02 = Predefined information) |
|  |  |  | (03 = Month) |
|  |  |  | (04 = Day) |
|  |  |  | (05 = Hour) |
|  |  |  | (06 = Quarter) |
vvv = |  | 0-255 |  | (depending on uu see command group 44) |
initial value uuvvv = |  | 00000 |  | (no voice answer) |

It is required that the stated reference (uuvvv) has been recorded with a system telephone in accordance with the commands of group 44.

The voice references will be played in numerical order.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003