BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1946
Forced message after timeout

This command states if a CONNECT or ALERTING message shall be sent to network 8 seconds after CALL PROCEEDING. This is to stop timer T303 and force the originating network to through connect the B-channel in order to give the caller the possibility to hear tones or announcements provided by the terminating party. The choice of CONNECT or ALERTING is network dependent.

DMinimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003