BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2613
Signal time

This command defines the tone time per digit for digit sending with DTMF.

Value: 0-32768

N.B! |  | Tone time = 32768 means continuous tone sending (of first keyed digit). Intended for use when measuring the DTMF-signal.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003