BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x79
Loss Of I/O Port Message

Default definition: |  | ERROR + TRIG |
Used by block: |  | RP |
Category: |  | DESIGNER |

The code is used by RP’s with ports. A message sequence error has been detected in an output message flow, using IOMESS messages, or there are no free transmit buffers. A complete message from the CPU to the current I/O-port is lost.

- D1:
- D2:
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003