BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4502
Meaning of digits 1-4

When ordering predefined information from an extension the orderer shall state four digits for time indication.

Depending on which information is intended (1-7) these digits signify month + day, hour + minute(s) or day + month.

This command determines the type of data for the various information texts.

1 = |  | Preprogrammed text with date indication; mmdd : month + day

2 = |  | Preprogrammed text with time indication; hhmm : hours + minutes

3 = |  | Preprogrammed text with date indication; ddmm : day + month

The preprogrammed text is determined via command 4501 Predefined info.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003