BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1922
Through connection after SETUP to net?

This command states if the B-channel shall be through-connected immediately after SETUP to the net.

This is to give the caller the possibility to hear tones or announcements provided by the terminating party without any preannouncement (PROGRESS information) in the dialling phase.

Default value = NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003