BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0141
Relative sending level

The command is used to state the relative transmission level (Lo) in the analogue interface to ELU-A.

Valid data: |  | -12dBr to + 6dBr (steps: 0,1 dBr)

Default data: |  | - 3 dBr

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003