BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0xA5
CS-Message Buffer Sequence Error

Default definition: |  | ERROR |
Used by block: |  | SP |
Category: |  | DESIGNER |

The serial communication processor (SP) on the CPU board has received a CSMEEX command with a parameter, pointing out an unexpected message buffer number. CP shall send CSMEEX commands in consecutive message buffers.

- D1: Expected buffer number
- D2: Received buffer number
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003