BusinessPhone Communication Platform 4.0
Facility Description – General ASB 150 02

## Functionality of ASB 150 02 With/Without Connected FECU

Together with the introduction of the ASB 150 02 R9, a software licencing concept was introduced.

Most of the features which are introduced from the Software Release ASB 150 02 R9 upwards can only be enabled by a hardware device, the so called "Feature Enabling Circuit Unit" (FECU), which is connected to the CPU-D4.

Each major commercial release (e.g. BusinessPhone 250 / BusinessPhone 50 Version 3, Version 4, ...) has its own FECU series, covering several packages.

#### BusinessPhone 250 / BusinessPhone 50 - Version 3 (ASB 150 02 R9, R10)

FECU article number: KDUBS 130 06 / x (x = Package 1-10 )

Package 1: |  | Basic Functions R9, R10

Package 2: |  | Standard digital networking (QSIG + VPN) with max. 32 trunk interfaces

Package 3: |  | Standard digital networking (QSIG + VPN) with unlimited trunk interfaces

Package 4: |  | Full digital networking (QSIG + VPN + UUS) with max. 32 trunk interfaces

Package 5: |  | Full digital networking (QSIG + VPN + UUS) with unlimited trunk interfaces

Package 6: |  | CTI

Package 7: |  | Standard digital networking (QSIG + VPN) with max. 32 trunk interfaces + CTI

Package 8: |  | Standard digital networking (QSIG + VPN) with unlimited trunk interfaces + CTI

Package 9: |  | Full digital networking (QSIG + VPN + UUS) with max. 32 trunk interfaces + CTI

Package 10: |  | Full digital networking (QSIG + VPN + UUS) with unlimited trunk interfaces + CTI

#### BusinessPhone 250 / BusinessPhone 50 - Version 4 (ASB 150 02 R11)

FECU article number: KDUBS 130 07 / x (x = Package 1-10 )

Package 1: |  | Basic Functions R11

Package 2: |  | Standard digital networking (QSIG) with 32 trunk interfaces

Package 3: |  | Standard digital networking (QSIG) with unlimited trunk interfaces

Package 4: |  | Full digital networking (QSIG + VPN + UUS) with 32 trunk interfaces

Package 5: |  | Full digital networking (QSIG + VPN + UUS) with unlimited trunk interfaces

Package 6: |  | Full digital networking (QSIG + VPN + UUS) with 4 trunk interfaces + CTI

Package 7: |  | Standard digital networking (QSIG) with 32 trunk interfaces + CTI

Package 8: |  | Standard digital networking (QSIG) with unlimited trunk interfaces + CTI

Package 9: |  | Full digital networking (QSIG + VPN + UUS) with 32 trunk interfaces + CTI

Package 10: |  | Full digital networking (QSIG + VPN + UUS) with unlimited trunk interfaces + CTI

Features which were introduced in a Release earlier than ASB 150 02 R9 are always enabled, and therefore also accessible if no FECU is connected to the CPU-D4. Furthermore fault corrections to existing unprotected features, as well as small feature improvements are always enabled.

Only two features are excluded from this philosophy: These are the "BusinessLink for Novell" and "proprietary CT Interface", which were introduced in ASB 150 02 R8. To run the "BusinessLink for Novell" and "proprietary CT Interface" on the system with R9 Software or upwards, the related FECU (see following table) is required.

The Package 1 always represents the new basic functionality of the Release, which is of course also included in all packages with a higher index.

If you upgrade a system to a higher SW-Release, without changing the FECU although the new Release has its own FECU series (separate article number), the system will remain on the same feature level, except for those features that are unprotected.

The following table shows the functionality enabled in ASB 150 02 depending on the connected FECU:

Available FECUs:

- KDUBS 130 06 / 1-10 (ASB 150 02 R9, R10)
- KDUBS 130 07 / 1-10 (ASB 150 02 R11)
- KDUBS 130 12 / 1-10 (reserved for ASB 150 02 R12)

The entries in the table indicate the minimum Software Release requirement for the respective feature. All features marked with "X" were introduced in a Release earlier than ASB 150 02 R9:

Feature (Blatt 1 von 5) | no FECU (unprotcetd) | FECU KDUBS 130 xx
/1 | /2 | /3 | /4 | /5 | /6 | /7 | /8 | /9 | /10
Abbreviated no. dial.- common numbers | X |  |  |  |  |  |  |  |  |  |
Abbreviated no. dial.- individual numbers via key pad |  | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9
Abbreviated no. dial.- individual numbers via prog. key | X |  |  |  |  |  |  |  |  |  |
Account numbers | X |  |  |  |  |  |  |  |  |  |
ACD Group | X |  |  |  |  |  |  |  |  |  |
ACD Agent &Supervisor | X |  |  |  |  |  |  |  |  |  |
ACD-Display clerical time |  | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9
ACD - Fixed clerical time with clerical key |  | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9
ACD - Monitoring clerical timeouts |  | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9
ACD - Multiple call codes |  | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9
Alarm function | X |  |  |  |  |  |  |  |  |  |
Authority code | X |  |  |  |  |  |  |  |  |  |
Automatic callback | X |  |  |  |  |  |  |  |  |  |
Background music | X |  |  |  |  |  |  |  |  |  |
Automated Attendant | X |  |  |  |  |  |  |  |  |  |
Call metering | X |  |  |  |  |  |  |  |  |  |
Call metering - Austria |  | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11
Call p. up - common | X |  |  |  |  |  |  |  |  |  |
Call p. up - ext. group | X |  |  |  |  |  |  |  |  |  |
Call p. up - individual | X |  |  |  |  |  |  |  |  |  |
Call waiting indic. | X |  |  |  |  |  |  |  |  |  |
Camp on | X |  |  |  |  |  |  |  |  |  |
Clock and diary | X |  |  |  |  |  |  |  |  |  |
Common bell | X |  |  |  |  |  |  |  |  |  |
Conference | X |  |  |  |  |  |  |  |  |  |
Conn. state mess. | X |  |  |  |  |  |  |  |  |  |
CT - proprietary CT Interf.* |  |  |  |  |  |  | R9 | R9 | R9 | R9 | R9
CT - BusinessLink for Novell * |  |  |  |  |  |  | R9 | R9 | R9 | R9 | R9
CT - BusinessLink for Windows NT |  |  |  |  |  |  | R10 | R10 | R10 | R10 | R10
CT - BusinessLink for Win NT - only Support of OWS |  | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10
CT groups =< 8 * |  |  |  |  |  |  | R9 | R9 | R9 | R9 | R9
CT groups =< 16 |  |  |  |  |  |  | R11 | R11 | R11 | R11 | R11
CT - Enhanced CIL func. |  |  |  |  |  |  | R10 | R10 | R10 | R10 | R10
Desk Top Manager | X |  |  |  |  |  |  |  |  |  |
DISA | X |  |  |  |  |  |  |  |  |  |
Diversion direct | X |  |  |  |  |  |  |  |  |  |
Diversion on busy | X |  |  |  |  |  |  |  |  |  |
Div. on no reply | X |  |  |  |  |  |  |  |  |  |
Doorph. (answering) | X |  |  |  |  |  |  |  |  |  |
DTMF tones | X |  |  |  |  |  |  |  |  |  |
DTMF tones at inc. calls | R9 |  |  |  |  |  |  |  |  |  |
Fault indication | X |  |  |  |  |  |  |  |  |  |
Fax extension | R9 |  |  |  |  |  |  |  |  |  |
Fictive numbers (<16) | X |  |  |  |  |  |  |  |  |  |
Fictive numbers (<1000) |  | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11
Follow me | X |  |  |  |  |  |  |  |  |  |
Group hunting seriell | X |  |  |  |  |  |  |  |  |  |
Group hunting parallel |  | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11
Hot line | X |  |  |  |  |  |  |  |  |  |
Hotel facilities | X |  |  |  |  |  |  |  |  |  |
Immediate answer | X |  |  |  |  |  |  |  |  |  |
Information via Info-key | X |  |  |  |  |  |  |  |  |  |
Information via keypad |  | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9 | R9
Inquiry | X |  |  |  |  |  |  |  |  |  |
Integrated Cordless - A protocol | X |  |  |  |  |  |  |  |  |  |
Integrated Cordless - GAP protocol |  | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10
Intercom | X |  |  |  |  |  |  |  |  |  |
Intrusion | X |  |  |  |  |  |  |  |  |  |
ISDN BA & PRA | X |  |  |  |  |  |  |  |  |  |
ISDN S-interface | X |  |  |  |  |  |  |  |  |  |
ISDN Caller List |  | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10
ISDN DDI, AOC | X |  |  |  |  |  |  |  |  |  |
ISDN CLIP, COLP | X |  |  |  |  |  |  |  |  |  |
ISDN CLIR, COLR | X |  |  |  |  |  |  |  |  |  |
ISDN - CLIR override |  | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10
ISDN MCID, MSN, SUB | X |  |  |  |  |  |  |  |  |  |
ISDN - Point to MultiPoint |  | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11
Key system function | X |  |  |  |  |  |  |  |  |  |
Last ext.numb.redial | X |  |  |  |  |  |  |  |  |  |
Least Cost Routing | X |  |  |  |  |  |  |  |  |  |
Loudspeaker paging | X |  |  |  |  |  |  |  |  |  |
Mailbox-sys. comm. | X |  |  |  |  |  |  |  |  |  |
Mailbox-sys. indiv. | X |  |  |  |  |  |  |  |  |  |
Mailbox-sys. individual greeting |  | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11
Message-sys. voice | X |  |  |  |  |  |  |  |  |  |
Message-s. call me | X |  |  |  |  |  |  |  |  |  |
Message-sys. text | X |  |  |  |  |  |  |  |  |  |
Music on hold | X |  |  |  |  |  |  |  |  |  |
Music on hold- integrated |  | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11
Name selection | X |  |  |  |  |  |  |  |  |  |
National specific functions - Croatia Adaptation of CN numbering plan |  |  |  |  | R10 | R10 | R11 |  |  | R10 | R10
National specific functions - Spain: Ibercom Indicator |  |  | R10 | R10 | R10 | R10 | R11 | R10 | R10 | R10 | R10
National specific functions - Poland: Testcall | R10 |  |  |  |  |  |  |  |  |  |
National specific functions - Austria: Support of packet mode terminals |  | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11 | R11
Networking - Tie line traffic via anal. Trunks | X |  |  |  |  |  |  |  |  |  |
Networking - VPN service from PSTN | X |  |  |  |  |  |  |  |  |  |
Networking - digital - with QSIG |  |  | R9 | R9 | R9 | R9 |  | R9 | R9 | R9 | R9
Networking - digital - with UUS |  |  |  |  | R9 | R9 | R11 |  |  | R9 | R9
Networking - digital - with UUS mapped into GFP |  |  |  |  | R11 | R11 | R11 |  |  | R11 | R11
Networking - digital - MD 110 BC10 adaptions |  |  |  |  | R10 | R10 |  |  |  | R10 | R10
Networking - digital - Central. Operator |  |  |  |  | R11 | R11 | R11 |  |  | R11 | R11
Night service | X |  |  |  |  |  |  |  |  |  |
O&M - Swapping boards during operation |  | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10
O&M -Remote upgrading |  | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10
O&M - Cordless remote programming |  | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10 | R10
Paging | X |  |  |  |  |  |  |  |  |  |
Park.for com.access | X |  |  |  |  |  |  |  |  |  |
Parking individual | X |  |  |  |  |  |  |  |  |  |
Private trunk line | X |  |  |  |  |  |  |  |  |  |
Programmable and fixed keys | X |  |  |  |  |  |  |  |  |  |
Refer back | X |  |  |  |  |  |  |  |  |  |
Register recall in PSTN | R9 |  |  |  |  |  |  |  |  |  |
Reminder service | X |  |  |  |  |  |  |  |  |  |
Saved ext. no. redial | X |  |  |  |  |  |  |  |  |  |
Secretary function | X |  |  |  |  |  |  |  |  |  |
Supervision | X |  |  |  |  |  |  |  |  |  |
Tandem - Slave | X |  |  |  |  |  |  |  |  |  |
Tandem - Master | X |  |  |  |  |  |  |  |  |  |
Telephone directory | X |  |  |  |  |  |  |  |  |  |
Testcall for Poland | X |  |  |  |  |  |  |  |  |  |
Trunk line key | X |  |  |  |  |  |  |  |  |  |
Voice mail box, external | X |  |  |  |  |  |  |  |  |  |

X |  | Feature was introduced in a Release earlier than ASB 150 02 R9

* |  | The "proprietary CT Interface" and "BusinessLink for Novell" were already released in ASB 150 02 R8 and are always enabled on the CPU-D3. In conjunction with the CPU-D4 they require the FECU devices.

Revision: PC1 © Ericsson Enterprise 2003