BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0162
Terminal type

This command is used to define the terminal type connected to the analogue extension interface.

Valid values:

0 |  | Speech

1 |  | 3.1kHz audio, general, orig.non ISDN

2 |  | 3.1kHz audio, fax G3, orig.non ISDN

3 |  | 3.1kHz audio, modem, orig.non ISDN

Default value:

0 |  | Speech

The terminal is automatically defined as FAX EXTENSION, if option 2 is selected; in this case, some restrictions in the settings of the following facilities have to be concerned:

Additional information for option 3 (modem): Using this option in combination with ISDN-lines and analogue extensions leads to releasing of DTMF-registers after receiving call proceeding.

IMPORTANT NOTE: This option must not be used in combination with LCR!

#### Extension related facilities:

- conference
- call back
- break-in
- camp-on
- diversion
- follow me

#### Trunk related facilities:

- reroute position
- voice announcement

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003