BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2084
Type of network call handling

The command defines whether network calls shall be handled as internal or external (tie line) calls with corresponding categories.

Example: Rerouting categories (on busy) for actual incoming trunk shall be deactivated (internal call handling) to enable proper ‘call back on busy handling’ from the network side.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003