BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6007
Character set

The command defines which set of characters shall apply for the local-connected unit for the stated I/O-port .

0 = |  | The PABX's internal set of characters (no characters are converted)

1 = |  | US-ASCII

2 = |  | Swedish/Finnish ASCII

3 = |  | Character set 2 in printer ERICSSON 7111 (strapped for compatibility with IBM-PC) and character set 850 (Multilingual) for SOFTECH hotel computer

4 = |  | Danish/Norwegian ASCII

5-9 = |  | Undefined values

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003