BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4601
Record messages allowed?

Voice messages, voice information and voice answers are stored on “voice memory boards”, VMU.

This command determines whether voice messages may be recorded on the stated board.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003