BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1307
PTS-signal from parent exchange ?

The command is used to state whether the exchange shall wait for a proceed-to-send signal (PTS signal) from the parent exchange. See command 1404 Wait time before start to send digits when no PTS for wrong proceed-to-send signal if the exchange does not send any signal.

(Command 1308 PTS-signal from parent exchange = dial tone ? states whether the proceed-to-send signal is the dial tone. See also command 1013 Dial tone to extension ?, which states whether dial tone shall be sent to the extension.)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003