BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1102
Answering position at night

This command is used to determine the individual answering position of the trunk in a night-switched exchange for manual incoming calls (not used for DDI calls). An individual answering position is selected by programming its directory number. If the directory number is erased, the individual answering position will be deleted.

Incoming calls are always presented on those system telephones on which the trunk is represented by a button. This applies irrespective of whether a directory number has been programmed/not programmed as individual answering position.

Note

If the individual answering position has the initial value = individual:
PBX-operator number, command 4001 Alternative answer position “General PBX-operator's alternative answering position” will not be operative.

Note

When the individual answering position is deleted, always make sure that an alternative answering position has been programmed so that incoming calls can be presented.

Verify therefore: Commands 1104 Reroute position at night, 1407 Maximum hold time and command group 03.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003