BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2406
Digit for executive intrusion

If an extension encounters busy on a call to another extension, the extension can initiate intrusion by pressing a predetermined key.

This command is used to determine the digit to be used for intrusion.

Only extensions with a service category permitting initiation of intrusion are allowed to initiate (utilize) this facility. See command 3004 Intrusion.

Intrusion can only be executed, if the categories of both parties in the ongoing call permit intrusion. See commands 0107 Break-in allowed ? and 1007 Break-in allowed ?.

If the digit has been used previously for another facility, it will be erased for this facility, i.e. the “old” facility will be removed from the system. See the other commands in this command group.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003