BusinessPhone Communication Platform 4.0
Commands > Commands 9000...9999

## 9006
Maxringtime at the init extension for CBack calls

This command specifies the time during which the initiating extension is ringing at network Call Back calls.

This timer must be programmed to the same value in every PBX which makes use of network Call Back.

If this timer expires the call is released, the initiating PBX initiates cancellation of Call Back, the missions in initiating and supervised PBX are deleted and the Call Back has failed.

Values: |  | 1 sec.:

|  | 255 sec.

Initial Value: |  | 8 sec.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003