BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8734
Use AA in combination with ACD group

This command will be used when the facility “CTI Groups” shall be used as a call filter in front of an ACD group. The command states whether the facility “CTI Groups” is used in combination with an ACD group or not. The parameter is the directory number of an ACD group. If there shall be no association with an ACD group the field is left blank. If a valid directory number of an ACD group is entered, the Automated Attendant will send MS-reports to a connected MS-PC if an ACD call has been rerouted by CTI.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003