BusinessPhone Communication Platform 4.0
Start Of Operation ASB 150 02

## Prerequisites

- The skilled technician should be familiar with the PBX in terms of location of the switches on the boards and the settings by RASC.
- The system shall be mounted. Presently two systems are available and connected in accordance with:

- “Installation Instruction” (1531‑BDV 113 08 Uen) for the BP 250 and
- “Installation Instruction” (1531‑BDV BS 101 01 Uen) for the BP 50.

- A personal computer installed with the maintenance program RASC (Remote Access Supervision and Configuration, LZY 203 2250), and Integrated Cordless System Manager Software program (LZYNB 201 01) should be available.
- To connect the computer with the system, use cord set TSR 902 0448/1 (PC and printer cable).

Revision: G © Ericsson Enterprise 2003