BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2221
PSTN-operator call numbers

This command is used to define which numbers are used for PSTN-operator calls.

Note

This command is only valid if command 1302 Outgoing digit transmission is set to MFE register signalling.

Value: 10 three-digit call numbers

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003