BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1312
MFC signal scheme

The command is used to state the signalling table for MFC (MFE/MFP) register signalling.

0 = |  | Standard R2

1 = |  | Simplified R2

2 = |  | Finnish R2

3 = |  | Norwegian R2

4 = |  | Mexican R2

5 = |  | Australien R2

6 = |  | Belgian simpl.R2

7 = |  | Malaysia R2

8 = |  | Brazil R2

9 = |  | Brazil LME

10 = |  | China R2

11 = |  | Israel R2

Value = 00-15

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003