BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4302
Max time for speech info

Voice messages, voice information and voice answers are stored on “voice memory boards”, VMUs.

To utilise the storage capacity of the board in the best possible manner it is possible, via commands 4301 Max time for speech message-4303 Max time for speech anno, to determine the duration of voice messages, voice information and voice answers.

This command determines the duration of each voice information.

1-255 = |  | Maximum duration in seconds

0 = |  | No voice information may be recorded

In addition to the programmed time the remaining (unused) storage capacity of the board determines the maximum time.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003