BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2002
Tone signal scheme

The tone signal scheme controls the frequency and cadence of each tone message.

0 = |  | Standard (CCITT)

1 = |  | Sweden

2 = |  | Australia

3 = |  | Finland

4 = |  | Denmark

5 = |  | Norway

6 = |  | Belgium

7 = |  | New Zealand

8 = |  | New Zealand with disconnection tone

9 = |  | Switzerland

10-99 |  | Not defined (standard CCITT will be used)

Note

Normally the PABX shall also be equipped with a market-adapted EXU-board in order to obtain the correct tone frequencies and levels

Revision: A © Ericsson Enterprise 2003